**1.16 - BIT ADDITION(8086)**

**PROGRAM:**

MOV SI,200H

LODSW

MOV BX,AX

LODSW

ADD BX,AX

MOV DI,1300H

MOV [DI],BX

HLT

**2.16 – BIT SUBTRACTION:**

**PROGRAM:**

MOV SI,1200H

LODSW

MOV BX,AX

LODSW

SUB BX,AX

MOV DI,1300H

MOV [DI],BX

HLT